error: invalid-instructions.asm(1):
    Address $10000 is not 16-bit
error: invalid-instructions.asm(2):
    LD [HL], [HL] is not a valid instruction
error: invalid-instructions.asm(3):
    Base value must be equal to $FF00 for $FF00+C
error: invalid-instructions.asm(4):
    syntax error, unexpected c, expecting hl
error: invalid-instructions.asm(5):
    syntax error, unexpected bc, expecting hl
error: invalid-instructions.asm(6):
    syntax error, unexpected number, expecting hl
error: invalid-instructions.asm(7):
    Bit number must be between 0 and 7, not 8
error: invalid-instructions.asm(8):
    Invalid address $40 for RST
error: Assembly aborted (8 errors)!
